# LifecycleStateTransitionType (Complex Type)

### Namespace: http://midpoint.evolveum.com/xml/ns/public/common/common-3

Specification of lifecycle state transition. EXPERIMENTAL

Item Summary
Name | Type | Multiplicity | Description
--- | --- | --- | ---
name | property string | [0,1] | Short name for the transition.
description | property string | [0,1] | Free-form description of transition purpose, mechanisms, etc.
documentation | property string | [0,1] | Technical documentation for a particular object or construct.
targetState | property string | [1,1] | Identifier of the state that is the target of the transition.
condition | property ExpressionType | [0,1] | Condition for automatic state transition.

- ### Items

  - #### name

    Flags: RAM,runtime

    Multiplicity: [0,1]

    Short name for the transition. It may be used in log files, user interface, etc.

  - #### description

    Flags: RAM,runtime

    Multiplicity: [0,1]

    Free-form description of transition purpose, mechanisms, etc. Used for documentation purposes (comment).

  - #### documentation

    Flags: RAM,runtime

    Multiplicity: [0,1]

    Technical documentation for a particular object or construct.

    The purpose of this element is to document system configuration and behavior. The documentation will not be presented to end users. In fact, it will probably not be presented at all in midPoint user interface. This documentation element is supposed to be a part of the technical documentation of midPoint deployment. The tools than generate deployment configuration will look for these elements and combine them to compiled documentation document.

    AsciiDoc formatting is assumed for this element. Any leading or trailing whitespace is skipped. Indentation equivalent to he indentation of the first non-blank line of text is also skipped.

  - #### targetState

    Flags: RAM,runtime

    Multiplicity: [1,1]

    Identifier of the state that is the target of the transition.

  - #### condition

    Flags: RAM,runtime

    Multiplicity: [0,1]

    Condition for automatic state transition. If the condition returns true value then lifecycle transitions to the target state.