# ActivityPolicyConstraintsType (Complex Type)

### Namespace: http://midpoint.evolveum.com/xml/ns/public/common/common-3

Supertype: AbstractPolicyConstraintType
Set of governance, risk management, compliance (GRC) and similar policy constraints related to tasks. These constraints act as triggers for the rules.

Item Summary
Name | Type | Multiplicity | Description
--- | --- | --- | ---
name | property string | [0,1] | Identifier of the constraint.
description | property string | [0,1] |
documentation | property string | [0,1] | Technical documentation for a particular object or construct.
presentation | container PolicyConstraintPresentationType | [0,1] | How should be triggering of this constraint presented, e.
executionTime | container DurationThresholdPolicyConstraintType | [0,1] | The execution time constrain evaluates activity execution time.
executionAttempts | container NumericThresholdPolicyConstraintType | [0,1] | This constraint evaluates how many times the activity realization was attempted.
itemProcessingResult | container ItemProcessingResultPolicyConstraintType | [0,1] | Constraint that evaluates result of one item (object) that was processed by activity.
and | container ActivityPolicyConstraintsType | [0,-1] | Constraints that must all apply.
or | container ActivityPolicyConstraintsType | [0,-1] | Constraints from which at least one must apply.
not | container ActivityPolicyConstraintsType | [0,-1] | The inner constraint must not apply.

- ### Items

  - #### name

    Flags: RAM,runtime

    Multiplicity: [0,1]

    Display order:

    Identifier of the constraint. It is used when midPoint needs to refer to a specific constraint, e.g. in order to record exception. This element is formally specified as optional, mostly due to the compatibility reasons. But it has to be provided in order for some functionality to work correctly.

  - #### description

    Flags: RAM,runtime

    Multiplicity: [0,1]

    Display order:

  - #### documentation

    Flags: RAM,runtime

    Multiplicity: [0,1]

    Display order:

    Technical documentation for a particular object or construct.

    The purpose of this element is to document system configuration and behavior. The documentation will not be presented to end users. In fact, it will probably not be presented at all in midPoint user interface. This documentation element is supposed to be a part of the technical documentation of midPoint deployment. The tools than generate deployment configuration will look for these elements and combine them to compiled documentation document.

    AsciiDoc formatting is assumed for this element. Any leading or trailing whitespace is skipped. Indentation equivalent to he indentation of the first non-blank line of text is also skipped.

  - #### presentation

    Flags: RAM,runtime

    Multiplicity: [0,1]

    Display order:

    How should be triggering of this constraint presented, e.g. in enforcement messages, in approvals, in certification, in notifications, etc.

  - #### executionTime

    Flags: RAM,runtime

    Multiplicity: [0,1]

    Display order:

    The execution time constrain evaluates activity execution time. When the exceeds element is specified, constraint will trigger if the task execution time exceeds the specified value. When the below element is specified, constraint will trigger if the task execution time is below the specified value.

  - #### executionAttempts

    Flags: RAM,runtime

    Multiplicity: [0,1]

    Display order:

    This constraint evaluates how many times the activity realization was attempted. When the "exceeds" element is specified, constraint will trigger if the number of attempts exceeds the specified value. When the "below" element is specified, constraint will trigger if the number of attempts is below the specified value.

  - #### itemProcessingResult

    Flags: RAM,runtime

    Multiplicity: [0,1]

    Display order:

    Constraint that evaluates result of one item (object) that was processed by activity.

  - #### and

    Flags: RAM,runtime

    Multiplicity: [0,-1]

    Display order:

    Constraints that must all apply. (But note that if there are more values of this item, they are interpreted according to the enclosing operator.)

  - #### or

    Flags: RAM,runtime

    Multiplicity: [0,-1]

    Display order:

    Constraints from which at least one must apply. (But note that if there are more values of this item, they are interpreted according to the enclosing operator.)

  - #### not

    Flags: RAM,runtime

    Multiplicity: [0,-1]

    Display order:

    The inner constraint must not apply.