# PhysicalMailingAddressType (Complex Type)

### Namespace: http://midpoint.evolveum.com/xml/ns/public/common/common-3

Information about a particular physical mailing address. It is modeled after RFC 7643 (System for Cross-domain Identity Management: Core Schema).

Item Summary
Name | Type | Multiplicity | Description
--- | --- | --- | ---
type | property string | [0,1] | Type of the address, like work, home, etc.
primary | property boolean | [0,1] | Is this the primary address (in a given context, e.
formatted | property string | [0,1] | The full mailing address, formatted for display or use with a mailing label.
streetAddress | property string | [0,1] | The full street address component, which may include house number, street name, P.
locality | property string | [0,1] | The city or locality component.
region | property string | [0,1] | The state or region component.
postalCode | property string | [0,1] | The zip code or postal code component.
country | property string | [0,1] | The country name component.

- ### Items

  - #### type

    Flags: RAM,runtime

    Multiplicity: [0,1]

    Display order:

    Type of the address, like work, home, etc. TODO lookup table here

  - #### primary

    Flags: RAM,runtime

    Multiplicity: [0,1]

    Display order:

    Is this the primary address (in a given context, e.g., for a user)?

  - #### formatted

    Flags: RAM,runtime

    Multiplicity: [0,1]

    Display order:

    The full mailing address, formatted for display or use with a mailing label. It may contain newlines.

  - #### streetAddress

    Flags: RAM,runtime

    Multiplicity: [0,1]

    Display order:

    The full street address component, which may include house number, street name, P.O. box, and multi-line extended street address information. It may contain newlines.

  - #### locality

    Flags: RAM,runtime

    Multiplicity: [0,1]

    Display order:

    The city or locality component.

  - #### region

    Flags: RAM,runtime

    Multiplicity: [0,1]

    Display order:

    The state or region component.

  - #### postalCode

    Flags: RAM,runtime

    Multiplicity: [0,1]

    Display order:

    The zip code or postal code component.

  - #### country

    Flags: RAM,runtime

    Multiplicity: [0,1]

    Display order:

    The country name component. When specified, the value MUST be in ISO 3166-1 "alpha-2" code format; e.g., the United States and Sweden are "US" and "SE", respectively.